|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| VP200 and VP220 Programming sheet | | | | | | |
| **Channel One** |  | | | | | |
| **WB or NB?** |  |  | | | | |
| **Tone A** |  | | | | | |
| **Tone B** |  | | | | | |
|  |  | | | | | |
| **Channel Two** |  | | | | | |
| **WB or NB?** |  |  | | | | |
| **Tone A** |  | | | | | |
| **Tone B** |  | | | | | |
|  |  | | | | | |
|  | Selective Call | Priority Scan | Monitor Mode | Normal Scan | Silent Scan |  |
| **Position A** |  |  |  |  |  |  |
| **Position B** |  |  |  |  |  |  |
| **Position C** |  |  |  |  |  |  |
| **Position D** |  |  |  |  |  |  |
|  |  | | | | | |
|  | BEEP | VIBE | BEEP AND VIBE |  | | |
| **Position A** |  |  |  |
| **Position B** |  |  |  |
| **Position C** |  |  |  |
| **Position D** |  |  |  |
|  |  | | | | | |
|  |
|  | ON | OFF |  | | | |
| **Voice Prompts** |  |  |
|  | ENABLE | DISABLE |
| **Squelch Method** |  |  | Enable squelch control record method | | | |
|  | 4  120 seconds | 8  60 seconds | 16  30 seconds | 32  15 seconds |  |  |
| **Time Storage** |  |  |  |  |  |  |
|  |  |  |  |  |  |  |