|  |
| --- |
| VP200 and VP220 Programming sheet |
| **Channel One** |  |
| **WB or NB?** |  |  |
| **Tone A** |  |
| **Tone B** |  |
|  |  |
| **Channel Two** |  |
| **WB or NB?** |  |  |
| **Tone A** |  |
| **Tone B** |  |
|  |  |
|  | Selective Call | Priority Scan | Monitor Mode |  Normal Scan | Silent Scan |  |
| **Position A** |  |  |  |  |  |  |
| **Position B** |  |  |  |  |  |  |
| **Position C** |  |  |  |  |  |  |
| **Position D** |  |  |  |  |  |  |
|  |  |
|  | BEEP | VIBE | BEEP AND VIBE |  |
| **Position A** |  |  |  |
| **Position B** |  |  |  |
| **Position C** |  |  |  |
| **Position D** |  |  |  |
|  |  |
|  |
|  | ON | OFF |  |
| **Voice Prompts** |  |  |
|  | ENABLE | DISABLE |
| **Squelch Method** |  |  | Enable squelch control record method |
|  | 4 120 seconds | 860 seconds | 1630 seconds | 3215 seconds |  |  |
| **Time Storage** |  |  |  |  |  |  |
|  |  |  |  |  |  |  |